

**Englewood Birch Specifications**

|  |  |
| --- | --- |
| Species | Birch |
| Size | 5”x3/8”xRL |
| Top Layer | 1.5 mm |
| Sqft per ctn | 29.12 |
| Lengths | 18”-48” |
| Construction | Engineered- Tongue and Groove |
| Plies | 5 |
| Style | Hand Scraped |
| Finish | 7 layer UV Coating |
| Edges | T&G eased edge |
| Installation | Staple, Nail, Glue, or Float |
| Warranty | 50 year finish & lifetime structure |