

**Francisco Euro Oak Specifications**

|  |  |
| --- | --- |
| Species | White Oak |
| Size | 7 ½”x ½” |
| Top Layer | 2 mm |
| Sqft per ctn | 30.43 |
| Lengths | RL up to 6’ |
| Construction | Engineered- Tongue and Grove |
| Plies | 6 |
| Style | Hand Scraped |
| Finish | 7 layer UV Coating |
| Edges | T&G eased edge |
| Installation | Staple, Nail, Glue, or Float |
| Warranty | 50 year finish & lifetime structure |