

**Grand Haven Specifications**

|  |  |
| --- | --- |
| Species | Hickory |
| Size | 3/8" x 3, 5, 7 |
| Top Layer | 1.5 mm |
| Sqft per ctn | 29.53 |
| Lengths | RL |
| Construction | Engineered- Tongue and Grove |
| Plies |  |
| Style | Hand Scraped |
| Finish | 7 layer UV Coating |
| Edges | T&G eased edge |
| Installation | Staple, Nail, Glue, or Float |
| Warranty | 50 year finish & lifetime structure |