

Vinyl Plank & Tile Specifications

**2mm Dryback- Newport**

|  |  |
| --- | --- |
| Size | 6”x48” |
| Thickness | 2 mm |
| Wear Layer | 8 mil |
| Gloss Level | 15 |
| Package | 36 sqft per carton / 60 ctns per pallet |
| Warranty | 25 Year Residential/ 10 Year Light Commercial |

**3.2mm Locking- Avalon**

|  |  |
| --- | --- |
| Size | 6”x48” |
| Thickness | 3.2 mm |
| Wear Layer | 8 mil |
| Gloss Level | 15 |
| Package  | 32 sqft per carton / 60 ctns per pallet |
| Warranty | 25 Year Residential/ 10 Year Light Commercial |

**6.5mm WPC Locking- Florence**

|  |  |
| --- | --- |
| Size | 7”x48” |
| Thickness | 6.5 mm |
| Wear Layer | 20 mil |
| Gloss Level | 15 |
| Package | 23.33 sqft per carton / 65 ctns per pallet |
| Warranty | Lifetime Residential/ 10 Year Light Commercial |

**6.5mm WPC Tile Locking- Coronado**

|  |  |
| --- | --- |
| Size | 12”x24” |
| Thickness | 6.5 mm |
| Wear Layer | 20 mil |
| Gloss Level | 15 |
| Package | 20 sqft per carton / 60 ctns per pallet |
| Warranty | Lifetime Residential/ 10 Year Light Commercial |