

**Tennessee Ridge Specifications**

|  |  |
| --- | --- |
| **Species** | **Oak** |
| **Sizes** | **2 ¼” or 3 ¼” x ¾” x RL** |
| **Sqft per ctn** | **2 ¼” – 25 sqft/ctn3 ¼” – 27 sqft/ctn** |
| **Finish** | **Aluminum Oxide** |
| **Style** | **Smooth Face** |
| **Lengths** | **9”-84” (average 32”)** |
| **Installation** | **Nail/ Staple** |
| **Application** | **Above Grade/ On Grade** |
| **Warranty** | **Lifetime Finish and Structure** |